# Motorola® Commercial Series Customer Programming Software

## English 中文

### Table of Contents

1. Introduction

2. What's new in this release

3. Requirements

4. Installation, upgrade, removal

5. Important notes

6. Legal notice

### 1. Introduction

Welcome to the Motorola Commercial Series Customer Programming Software (CPS) for the GP3188, GP3688, GM3188, GM3688, GM3189, GM3689 and GP3689 radios.

### 2. What's new in this release

Version | Notes
R05.16 | Support 403-445MHz on GP3188 H50ZDC9AJ2AN.
| Support 138 channels on GM3688 M50ZNF9AA2AN.
R05.15 | Support ELP Refresh PTT Side Tone and Radio Lock Enhancement
R05.13 | Support the following feature enhancements in Conventional radio: Clip Frequency to 438MHz.
R05.09 | Same as R05.08.
R05.08 | Support Self Test Report feature.
R05.07 | Support India models which only allow 12.5KHz Channel Bandwidth setting. Support ‘Selected Channel Lock’ and ‘Priority Channel 1 Lock’ features.
R05.06 | Support Flat Tx Audio feature.
R05.05 | Fixed Talk Around issue. Support scroll bar feature.
R05.04 | Support Radio ID, Vote Scan, and Call Alert features. Support GP3689 radios. Extending 5MHZ into the upper end of the UHF1 band which covers 403-445MHz (only for Korea due to regulation changes).
R05.03 | Fix Selective Call feature version issue.
R05.02 | Support MDC Selective Call feature.
R05.01 | Support new models of GP3688 radios with Sales Model No. CMHxxxxxxxxx.
| Support character 'P' as Pause Character in phone number for radios with codeplug version 03.xx and above.
| Support 100 personalities on GM3189.
| Fixed the 12.5 KHz channel frequency issue of GM3189/GM3689.
| CPS automatically modifies codeplug mismatched values when reading archive files of radios with firmware versions R02.00.xx and prior.
| Support GM3688 with Model No. AZM50NNF9AA2.
R05.00 | Support for GP3688 radios with Sales Model No. CMHxxxxxxxxx.
R04.00 | Support GM3189 and GM3689 radios.
| The channel position was under 'Conventional Personalities' in the old CPS and is now moved to the left window under a new item called 'Channel Position'.
R02.05 | Support for Designated Power Up Channel.
R02.04 | Fixed cloning issues between different codeplug versions.
| Support for additional frequency bands for the GM3188 and GM3688 radios.
R02.01 | Modified the transmit power calculation for the GM3188 and GM3688 radios.
R02.00 | Support for GP3688 and GM3688 radios.
| Drag and drop support and cloning support between different codeplug versions.
| Support for copying the receive frequency, with an optional user defined offset, to the transmit frequency.
R01.02 | Support for new serial number format from factory.
| Improved error handling during radio communication.
R01.01 | Now supports synthesizer step sizes of 2.5 kHz. This is necessary to support certain narrowband (12.5 kHz) frequencies.
| Now supports per user settings for the preference settings and the dealer information fields printed on the customer handout report.
R01.00 | Support for the GP3188 and GM3188 radios.
| Drag and drop support between models and products.
| Support for renaming personalities, systems, and lists.
| Support for multiple selection configuration. For example, create several MDC systems and select them all in the treeview and set the Primary ID of all the MDC systems to the same value at once.

### 3. Requirements

Operating System | Required Patches
Microsoft® Windows® 98 First Edition | Windows 98 Year 2000 Update
| Windows 98 Year 2000 Update 2
| System Update
Microsoft® Windows® 98 Second Edition |
Microsoft® Windows® Millennium Edition |
Microsoft® Windows® NT 4.0 | SP5 or greater, excluding SP6 (SP6a is supported).
Microsoft® Windows® 2000 Professional |
Microsoft® Windows® XP Home/Professional Edition |
Microsoft® Windows® 7 |

Hardware Recommendations
· The application takes approximately 16 MB of free disk space on your PC. However, you may want more space to allow you to save archive files of your radios. Each archive file varies in size depending on the features of the radio that are enabled. A good rule of thumb is 75 KB per archive file.
· For processor speed and RAM, nothing is required beyond the recommendations given by Microsoft for the release of the operating system that you are using.
· The graphical user interface is best displayed using 1024*768 and 65536 color display or better (use small font).
· A CD-ROM drive.
· A serial port or USB to serial port adapter. The BAFO(R) BF-810 USB to serial port adapter has been tested successfully with the CPS application.

### 4. Installation, Upgrade, Removal

#### Installation

You need to have Administrator rights on the target PC in order to install the software if you are running Microsoft Windows NT 4.0, Microsoft Windows 2000 Professional, or Microsoft Windows XP Home/Professional Edition.

Proceed as follows for CD-ROM version:

- Insert the CD-ROM containing the installation into the CD-ROM drive.
- If the installation application doesn't start within 30 seconds, the auto-run feature for CD-ROMs for you operating system is likely disabled. Browse to your CD-ROM and run the setup.exe program. For example, if the E:\ drive is the CD-ROM, run E:\ setup.exe.
- If a previous version of CPS has already been installed, you will be given the option to “Repair” or “Remove”. If you are upgrading the CPS, then remove the previous version and start the installation process again. If you are re-installing the CPS, then choose the repair option.

Proceed as follows for software package version:

- Unzip the CPS package to a directory of a local disk.
- Browse to this directory and run the setup.exe program.
- If a previous version of CPS has already been installed, you will be given the option to “Repair” or “Remove”. If you are upgrading the CPS, then remove the previous version and start the installation process again. If you are re-installing the CPS, then choose the repair option.

#### Upgrade

During the upgrade procedure, settings for preferences and dealer information will be reset to their default values. You will need to check these settings after the new version has been installed and make changes as necessary.

To upgrade from a previous version of this software, first remove the previous version (see instructions in section below) and then install this version.
This version can open any archive file created with a previous versions. In addition, it supports all previously released codeplug versions so you will be able to read, write, and clone older radios as well.

#### Removal

From the Start button on the task bar of your operating system, select Settings > Control Panel. Select the Add/Remove Programs option within the control panel. Select the Commercial Series Customer Programming Software item in the "Currently installed programs" box and click the remove button.

### 5. Important Notes

The following issues are known problems with the latest release of the Motorola Commercial Series CPS.

- If the display setting's font size is set to "Custom setting" instead of "Small Fonts" or "Large Fonts" the Toolbar and Conventional Personalities folder may not display properly.
- The installation doesn't set the default path to save archive files and therefore the user will need to migrate to the directory of their choosing the first time they save a file.
- In order to use the CPS in Chinese on Microsoft Windows 2000 and Microsoft Windows XP, please verify the locale under regional option is configured to Chinese (PRC) and the default language setting for system under regional option is configured to Simplified Chinese. To verify the regional option, navigate to the following location:Start -> Settings -> Control Panel -> Regional Options.

### 6. Legal notice

Microsoft® and Windows® are registered trademarks of Microsoft Inc.
Motorola® is a registered trademark of Motorola, Inc.
BAFO® is a registered trademark of BAFO Technologies, Inc.
ARTS® is a registered trademark of Vertex Standard.
This product includes software developed by the Apache Software Foundation (http://www.apache.org/). For more information, please refer to MOTOROLA_PAS_LEGAL_NOTICES_EULA_FILE-CPS.

### 目录:

1. 简介

2. 此版本所做更新

3. 系统要求

4. 安装，升级，卸载

5. 重要注意事项

6. 法律声明

### 1. 简介

欢迎使用摩托罗拉 Commercial Series Customer Programming Software (CPS)。本软件支持GP3188, GP3688, GM3188和GM3688等对讲机。

### 2. 此版本所做更新

版本 | 说明
R05.16 | 支持频率范围为403-445MHz模型号为H50ZDC9AJ2AN的GP3188对讲机。
| 支持138信道模型号为M50ZNF9AA22AN的GM3688对讲机。
R05.15 | 在常规对讲机上增强如下功能: 电台长锁以及ARTS侧音。
R05.13 | 在常规对讲机上支持如下新加入的功能: 限制频率为438Mhz。
R05.09 | 同R05.08。
R05.08 | 支持开机自检报告功能。
R05.07 | 支持‘选择信道锁定’和‘优先级信道1锁定’功能。
R05.06 | 支持平滑发射音频功能。
R05.05 | 解决了Talk Around 问题。 支持鼠标滚轮。
R05.04 | 支持 Radio ID, Vote Scan, 和 Call Alert 功能。 支持GP3689 对讲机。
R05.03 | 解决了MDC选择性呼叫版本支持问题。
R05.02 | 支持MDC选择性呼叫功能。
R05.01 | 支持GP3688对讲机的新型号。（销售型号为CMHxxxxxxxxx）。
| 支持在电话号码中输入'P'为暂停字符，适用于Codeplug版本03.xx 及以上的对讲机。
| 在读入固件版本为02.xx或以下的CPS存档文件时自动修复不一致的codeplug值。
| 支持模型号为AZM50NNF9AA2的GM3688对讲机。
R05.00 | 支持销售型号为CMHxxxxxxxxx的GP3688对讲机。
R04.00 | 升级至版本4。左视图中"常规信道"节点下的信道位置表被移动到左视图的新节点“信道位置“下。
R02.05 | 支持上电信道。
R02.04 | 解决了不同版本codeplug复制过程中存在的错误。
| 支持对讲机GM3188和GM3688的附加频段。
R02.01 | 修改了对讲机GM3188和GM3688发射功率的计算方法。
R02.00 | 支持对讲机GP3688和GM3688。
| 支持不同版本codeplug之间的拖放和复制。
| 支持用接收频率加上用户指定的偏移量来自动生成发射频率。
R01.02 | 支持工厂新的序列号格式。
| 改进了对讲机通信过程中的错误处理。
R01.01 | 支持步长为2.5kHz的频率合成器，这对支持某些窄带频率(12.5 kHz)是必需的。
| 各个用户可以有自定的参数设置，支持在用户手册上打印经销商的信息。
R01.00 | 支持对讲机GP3188 和GM3188。
| 支持不同型号和产品间的拖放功能。
| 支持重命名常规信道、系统和列表。
| 支持多项选择并同时进行配置。例如在创建多个MDC系统后，在左边的树状视图中将它们全部选中，然后同时为所有的MDC系统设置相同的主ID。

### 3. 系统要求

操作系统 | 必需的补丁
Microsoft® Windows® 98 第一版 | Windows 98 Year 2000 Update
| Windows 98 Year 2000 Update 2
| 系统升级
Microsoft® Windows® 98 第二版 |
Microsoft® Windows® Millennium Edition （即Windows ME） |
Microsoft® Windows® NT 4.0 | SP5 或更高版本，但不包括SP6 (支持 SP6a)。
Microsoft® Windows® 2000 专业版 |
Microsoft® Windows® XP 家庭/专业版 |
Microsoft® Windows® 7 |

推荐硬件
· 这一应用程序需要占用PC上大约16MB的磁盘空间。但是，你需要更多的磁盘空间来保存对讲机的数据存档文件。根据对讲机支持的功能的不同，各个存档文件的大小可能不同。一个简略的估算方法是：每个文件75KB。
· 对于处理器速度和内存无特殊要求， 只要满足Microsoft推荐的能正常运行操作系统的条件即可。
· 图形用户界面在1024 ´768像素、65536色(使用小字体)的设置下效果最佳。
· 一个CD-ROM驱动器。
· 一个串口或USB接口。BAFO(R) BF-810 USB接口已成功地通过测试。

### 4. 安装，升级，卸载

#### 安装

如果使用的是Microsoft Windows NT 4.0, Microsoft Windows 2000专业版，或Microsoft Windows XP家庭/专业版，那么需要PC的管理员权限才能安装该软件。

按以下步骤操作： （光盘版）

- 把安装光盘插入CD-ROM驱动器。
- 如果安装程序在30秒内没有启动，那么很有可能是你的操作系统关闭了CD-ROM的自动运行功能。浏览你的CD-ROM并运行setup.exe。例如：如果E: 是CD-ROM，那么就运行E:\ setup.exe。
- 如果以前已经安装了此CPS，那将会出现两个选项：“修复”和“删除”。如果你要升级CPS，那么请选择删除选项来删除旧版本的CPS，然后再重新开始此安装流程。如果你要重新安装CPS, 那么请选择修复选项。

按以下步骤操作： （安装包版）

- 将CPS安装包解压到本地磁盘的一个目录。
- 浏览该目录并运行setup.exe。
- 如果以前已经安装了CPS，将会出现两个选项：“修复”和“删除”。如果要升级CPS，请选择删除选项先删除旧版本的CPS，然后再重新开始此安装流程。如果要重新安装CPS, 那么请选择修复选项。

#### 升级

在升级的过程当中，“参数选择”和“经销商信息”中的设置将会被恢复为缺省值。在新版软件安装完毕之后你需要检查这些设置，并进行必要的修改。

在升级软件之前，先卸载旧版本的软件（参见下一部分的说明），然后再安装新版的软件。这一版本的软件可以打开旧版的所有存档文件，并支持之前发布的所有版本的codeplug，因此，可以对旧版的对讲机进行读、写和克隆。

#### 卸载

点击操作系统“任务栏”的“开始”按钮，选择“设置”>“控制面板”>“添加/删除程序”选项。在“当前已安装程序”中选中“Commercial Series Customer Programming Software”，然后点击“卸载”按钮。

### 5. 重要注意事项

Motorola Commercial Series CPS 此版本存在以下一些已知的问题。

- 如果显示设置中的字体大小设置为“自定义字体大小”而不是“小字体”或“大字体”时，工具栏和常规信道视图的显示可能会不正常。
- 安装程序并没有设置保存存档文件的缺省路径，第一次保存文件时用户需要对文件路径进行相应设置。
- 如果要在Microsoft Windows 2000 和 Microsoft Windows XP下使用中文版的下CPS，请核实“区域选项”下的“区域设置”是否被设置为“中文（中国）”，“系统的语言设置”的缺省值是否被设置为“中文（简体）”。核实“区域选项”的方法是：点击“开始” >“设置”>“控制面板”> “区域选项”。

### 6. 法律声明

Microsoft® 和 Windows® 是Microsoft公司的注册商标。
Motorola® 是Motorola公司的注册商标。
BAFO® 是BAFO Technologies, Inc的注册商标。
ARTS® 是Vertex Standard的注册商标。
本产品内含由Apache Software Foundation (http://www.apache.org/)所开发的软件。更多信息，参见MOTOROLA_PAS_LEGAL_NOTICES_EULA_FILE-CPS.